{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["申报表"],"read":"whole","date_system":"1900"}

{"sheet":"申报表","index":0,"n_rows":239,"n_cols":8,"rows_kept":239,"merged":[[238,0,238,7]]}
["序号","专业名称/课程名称","实验(训)\n人数","货物名称","技术参数","单位","数量","备注"]
[1,"机电一体化综合实训",55,"电气网孔板","400mm*600mm，带提手","个",5]
[2,"机电一体化综合实训",55,"交流接触器","CJX2—1210","个",6]
[3,"机电一体化综合实训",55,"国标安装导轨","宽35mm，长30cm","个",6]
[4,"机电一体化综合实训",55,"桥型零线排","10孔","个",12]
[5,"机电一体化综合实训",55,"三插电源线","3芯电源线，1m，10A","根",6]
[6,"机电一体化综合实训",55,"PLC","FX3U-16MT/ES-A，SL,晶体管型","个",3]
[7,"单片机原理及接口技术",85,"开关电源","24V 3A","个",6]
[8,"单片机原理及接口技术",85,"熔断器","1P底座 2A","个",6]
[9,"单片机原理及接口技术",85,"中间继电器","8脚DC24+底座","个",6]
[10,"单片机原理及接口技术",85,"接线端子","导轨式接线端子 100片/盒","盒",6]
[11,"单片机原理及接口技术",85,"三插电源线","3芯电源线，1m，10A","根",9]
[12,"单片机原理及接口技术",85,"步进电机套装","含步进驱动器、丝杆滑台","个",6]
[13,"机械产品数字化设计",120,"批头十一字","65+110mm","支",2]
[14,"机械产品数字化设计",120,"专用多功能扳手","8寸GREENER","把",1]
[15,"机械产品数字化设计",120,"投影仪灯泡","原装高亮","个",2]
[16,"机械产品数字化设计",120,"排插","GN-B3043，1.8米","个",2]
[17,"机械产品数字化设计",120,"绘图笔芯","0.5mm黑色，每盒20支","盒",4,"3黑+1红"]
[18,"机械产品数字化设计",120,"温度断路器","KSD302（125℃）","个",6]
[19,"机械产品数字化设计",120,"电池","5#（15），7#（10）","个",25]
[20,"机械产品数字化设计",120,"电源适配器延长线","铜芯5.5*2.5mm公母头2.1","根",1,"3米加粗"]
[21,"机械产品数字化设计",120,"电脑系统安装盘","WIN11及以下，32/64位","个",1,"64G"]
[22,"机械产品数字化设计",120,"绘图油泥","红+黑","盒",2]
[23,"机械产品数字化设计",120,"数字化存储卡","512G，190MB/sV30","个",2]
[24,"机械产品数字化设计",120,"数字化输出器","D2421H，23.8， FHD","个",1]
[25,"机械产品数字化设计",120,"仪表箱","40*30*18CM，14L,2KG(丹秘黑)","个",1]
[26,"传感器",235,"插排","3个3插，3米","个",5]
[27,"传感器",235,"直流电源","120W-24V 5A","块",5]
[28,"传感器",235,"人机界面触摸屏","TPC7062Ti（带网口、2P电源插拔端子、DB9针接口）","台",4]
[29,"传感器",235,"传输线1","方型口USB数据下载线（1.5m）","根",4]
[30,"传感器",235,"网线","六类千兆（纯铜线芯，1.5m）","根",4]
[31,"传感器",235,"卷线","RV0.75,50米","卷",2]
[32,"传感器",235,"一字螺丝刀","3*75mm","个",6]
[33,"传感器",235,"万用表",null,"只",4]
[34,"传感器",235,"香蕉头导线","10cm长，0.75平方","根",120,"红黄黑各40"]
[35,"传感器",235,"香蕉头导线","50cm长，0.75平方","根",120,"红黄黑各40"]
[36,"传感器",235,"透明皂","102克*12块","袋",1]
[37,"电气控制技术",235,"铠装逆变器漆包线","QA-1/155度，线径0.35mm，重量5KG/捆","捆",2]
[38,"电气控制技术",235,"铠装整流器裸线","QZY-2/180 线径0.8mm 重量5KG/捆","捆",2]
[39,"电气控制技术",235,"国标电线","BV2.5国标铜芯线100M每卷","捆",3," 红色"]
[40,"电气控制技术",235,"国标电线","BV2.5国标铜芯线 100M每卷","捆",3,"黑色"]
[41,"电气控制技术",235,"国标电线","BV2.5国标铜芯线100M每卷","捆",3," 黄色"]
[42,"电气控制技术",235,"国标电线","BV2.5国标铜芯线100M每卷","捆",2," 绿色"]
[43,"电气控制技术",235,"国标电线","BV2.5国标铜芯线 100M每卷","捆",2,"蓝色"]
[44,"电气控制技术",235,"涤纶复合丝纤维抹布","40*60cm","块",5]
[45,"电气控制技术",235,"鹰嘴式剥线钳","剥线范围：0.5-3.3mm","把",5]
[46,"电气控制技术",235,"台式主机捆绑带","四维固定款","根",5]
[47,"电气控制技术",235,"三极空气开关","3P，10A","个",5]
[48,"电气控制技术",235,"单相有功电度表","型号: DDS666-5 (20）A","台",5]
[49,"汽车检测与维修技术",240,"穿心螺丝刀","一字 ，中号","把",4]
[50,"汽车检测与维修技术",240,"穿心螺丝刀","一字，大号","把",6]
[51,"汽车检测与维修技术",240,"方孔中轴拆装套筒","20齿","只",1]
[52,"汽车检测与维修技术",240,"亚克力门头标牌","银底黑字，“208”","个",2]
[53,"汽车检测与维修技术",240,"亚克力门头标牌","银底黑字，“204”","个",2]
[54,"汽车检测与维修技术",240,"亚克力门头标牌","银底黑字，“201”","个",2]
[55,"汽车检测与维修技术",240,"亚克力门头标牌","银底黑字，“203”","个",2]
[56,"汽车检测与维修技术",240,"车衣(半罩）","牛津，单层，灰色","套",10]
[57,"汽车检测与维修技术",240,"创可贴",null,"个",50]
[58,"汽车检测与维修技术",240,"推尘平板拖把","大号，120cm","把",6]
[59,"汽车检测与维修技术",240,"门绊锁扣","大号，挂锁用","个",5]
[60,"汽车检测与维修技术",240,"轮胎动平衡配重块","各种规格","套",2,"粘贴式"]
[61,"汽车检测与维修技术",240,"自动启停蓄电池","自动启停","只",1,"适配迈腾B8"]
[62,"汽车检测与维修技术",240,"蓄电池","6-QW-40(360)12V","只",1,"（适配比亚迪秦EV 22款）"]
[63,"汽车检测与维修技术",240,"蓄电池","fengfanL2-400","只",2]
[64,"汽车检测与维修技术",240,"汽修专业版启动电源","12V，X2500，8芯","台",1,"32000+加粗夹"]
[65,"汽车检测与维修技术",240,"24件套精密螺丝批","套装","套",3]
[66,"汽车检测与维修技术",240,"无油空气压缩机","18L，600W","台",2]
[67,"汽车检测与维修技术",240,"气鼓","15米吹尘管","台",2]
[68,"汽车检测与维修技术",240,"电鼓","15米，防水插座","台",2]
[69,"汽车检测与维修技术",240,"双层加厚工具箱","18寸","只",2]
[70,"汽车检测与维修技术",240,"剪刀","QHSS-185，长185cm","把",3]
[71,"汽车检测与维修技术",240,"纽扣电池",2032,"粒",10]
[72,"汽车检测与维修技术",240,"漆笔","白色","只",3]
[73,"汽车检测与维修技术",240,"冷媒开瓶器","通用","只",20]
[74,"汽车检测与维修技术",240,"双门双面玻璃门锁","外匙内拧铜芯","只",3]
[75,"汽车检测与维修技术",240,"4分软胶管水龙头接头","快接头，高质量","个",2]
[76,"汽车检测与维修技术",240,"水龙头快接头","4分，高质量","个",2]
[77,"汽车检测与维修技术",240,"汽车动平衡仪记录模块",null,"个",2]
[78,"汽车检测与维修技术",240,"四轮定位仪记录模块",null,"个",2]
[79,"汽车检测与维修技术",240,"白纱手套","棉","双",300]
[80,"汽车检测与维修技术",240,"一次性档把护套","4S店保养专用","包",100]
[81,"汽车检测与维修技术",240,"小型工具台","2抽1门，长40宽40高61","只",6]
[82,"汽车检测与维修技术",240,"工具电脑包（深灰色）","13寸笔记本，单肩带","只",1]
[83,"汽车检测与维修技术",240,"钢制货架","1.5米长，白色，4层","个",2]
[84,"汽车检测与维修技术",240,"PVC塑料储物盒","蓝色周转箱40*30*75cm","个",20]
[85,"汽车检测与维修技术",240,"6AT自动变速箱模型","可演示6+R档","套",1]
[86,"新能源汽车技术",380,"机盖保险丝盒总成","前舱配电盒","套",1,"适配19款比亚迪秦EV"]
[87,"新能源汽车技术",380,"汽车保险丝小号","全规格各种型号","片",100,"适配比亚迪秦EV"]
[88,"新能源汽车技术",380,"汽车保险丝迷你","全规格各种型号","片",100,"适配比亚迪秦EV"]
[89,"新能源汽车技术",380,"汽车保险丝长脚","全规格各种型号","片",100,"适配比亚迪秦EV"]
[90,"新能源汽车技术",380,"汽车保险丝方形","全规格各种型号","片",50,"适配比亚迪秦EV"]
[91,"新能源汽车技术",380,"汽车继电器",null,"只",10,"适配比亚迪秦EV"]
[92,"新能源汽车技术",380,"混动电机","秦dmi","只",2,"适配比亚迪"]
[93,"新能源汽车技术",380,"混动汽车轮毂电机",null,"套",1]
[94,"新能源汽车技术",380,"星型齿轮机构组模型",null,"套",2]
[95,"新能源汽车技术",380,"汽车模拟悬架","麦弗逊式","个",2]
[96,"新能源汽车技术",380,"汽车模型","01:32:00","辆",4]
[97,"新能源汽车技术",380,"汽车车身零件","01:18:00","个",6]
[98,"新能源汽车技术",380,"灯泡","直插式 氙气 H4 5000k白光（100W）","个",2]
[99,"新能源汽车技术",380,"雨刮","boshclear fit U型无骨14英寸/20英寸","套",1]
[100,"新能源汽车技术",380,"高压配电箱","充配电总成","个",2,"适配19款比亚迪秦EV"]
[101,"新能源汽车技术",380,"铅酸蓄电池","6-DZF-23","套",2]
[102,"新能源汽车技术",380,"发动机教学模型","中号 trent900 涡扇发动机","个",1]
[103,"新能源汽车技术",380,"机滤","MAHLE OC611","个",2]
[104,"新能源汽车技术",380,"扭力计","数显 PNC-135","个",1]
[105,"新能源汽车技术",380,"电动空调压缩机","高压","个",2,"适配19款比亚迪秦EV"]
[106,"新能源汽车技术",380,"铜丝刷","铁柄弯","把",5]
[107,"新能源汽车技术",380,"钢丝刷","铁柄弯","把",5]
[108,"新能源汽车技术",380,"变频电机驱动板","型号：200034","个",1]
[109,"新能源汽车技术",380,"台架数据输入器",null,"个",1]
[110,"新能源汽车技术",380,"新能源实训台架信号输入端子",null,"套",1]
[111,"新能源汽车技术",380,"机油","型号：0W20","桶",1]
[112,"新能源汽车技术",380,"汽车电路图","A4 正反面打印 胶装","本",4,"电路图中标后提供"]
[113,"新能源汽车技术",380,"不锈钢方形托盘","40cm x 50cm","个",2]
[114,"新能源汽车技术",380,"粉笔","无尘粉笔","盒",5]
[115,"新能源汽车技术",380,"电池","5号","只",40]
[116,"新能源汽车技术",380,"电池","7号","只",40]
[117,"新能源汽车技术",380,"油桶","200升黑色闭口烤漆","只",1]
[118,"新能源汽车技术",380,"机油","SN,4升，通用","桶",6,"二级维护"]
[119,"新能源汽车技术",380,"汽油","93＃","升",240]
[120,"新能源汽车技术",380,"汽油","95＃","升",60]
[121,"新能源汽车技术",380,"一次性手套","丁腈橡胶","双",50]
[122,"新能源汽车技术",380,"手套","A688 L码","双",24]
[123,"新能源汽车技术",380,"插线板","bull独立4插位5眼","个",4,"线长5米"]
[124,"《数控车削加工技术》",50,"CRCPR03262防锈润滑油","型号：CRC-03262 规格SP-350/311g","瓶",2]
[125,"《数控车削加工技术》",50,"CRC5-56防锈润滑剂","型号：CRC05005CW 规格5-56/410g","瓶",2]
[126,"《数控车削加工技术》",50,"CRC润滑剂","型号：CRC03044 规格283g","瓶",2]
[127,"《数控车削加工技术》",50,"CRC清洁剂","型号：PR05088CR 规格500ml/350g","瓶",2]
[128,"《数控车削加工技术》",50,"CRC除尘剂","型号：PR14085 规格227g","瓶",2]
[129,"《数控车削加工技术》",50,"CRC清洁剂","型号：PR02016C 规格300g","瓶",2]
[130,"《数控车削加工技术》",50,"智能数字万用表","ZTW8906，配充电套装，配特尖表笔","套",1]
[131,"《数控车削加工技术》",50,"1000W直流电源","LEADEX Ⅲ1000W 规格：ATX3.1","只",1]
[132,"《数控车削加工技术》",50,"特厚丁晴钻石纹一次性防护手套","INTCO 1009S，尺寸：L，规格：100只/盒","盒",6]
[133,"《数控车削加工技术》",50,"铝用车刀片","VCGT110304，规格：10片/盒","盒",1]
[134,"《数控车削加工技术》",50,"铝用车刀片","TNGC160404，规格：10片/盒","盒",1]
[135,"《数控车削加工技术》",50,"铝用车刀片","TNGC160404，规格：10片/盒","盒",1]
[136,"《车铣复合加工技术》",80,"整体钨钢硬质合金钻头","HDH5040300，尺寸：3mm，规格：5D-incool","支",1]
[137,"《车铣复合加工技术》",80,"整体钨钢硬质合金钻头","HDH5040330，尺寸：3.3mm，规格：5D-incool","支",2]
[138,"《车铣复合加工技术》",80,"整体钨钢硬质合金钻头","HDH5040400，尺寸：4mm，规格：5D-incool","支",2]
[139,"《车铣复合加工技术》",80,"整体钨钢硬质合金钻头","HDH5040420，尺寸：4.2mm，规格：5D-incool","支",2]
[140,"《车铣复合加工技术》",80,"整体钨钢硬质合金钻头","HDH5040500，尺寸：5mm，规格：5D-incool","支",2]
[141,"《车铣复合加工技术》",80,"整体钨钢硬质合金钻头","HDH5040600，尺寸：6mm，规格：5D-incool","支",2]
[142,"《车铣复合加工技术》",80,"整体钨钢硬质合金钻头","HDH50408500，尺寸：8.5mm，规格：5D-incool","支",2]
[143,"《车铣复合加工技术》",80,"整体钨钢三牙公制螺纹铣刀","WACK-M3*0.5，规格：3倍","支",1]
[144,"《车铣复合加工技术》",80,"整体钨钢三牙公制螺纹铣刀","WACK-M4*0.7，规格：3倍","支",1]
[145,"《车铣复合加工技术》",80,"整体钨钢三牙公制螺纹铣刀","WACK-M5*0.8，规格：3倍","支",1]
[146,"《车铣复合加工技术》",80,"整体钨钢三牙公制螺纹铣刀","WACK-M6*1.0，规格：3倍","支",1]
[147,"《车铣复合加工技术》",80,"整体钨钢三牙公制螺纹铣刀","WACK-M8*1.25，规格：3倍","支",1]
[148,"《车铣复合加工技术》",80,"整体钨钢三牙公制螺纹铣刀","WACK-M10*1.5，规格：3倍","支",1]
[149,"《车铣复合加工技术》",80,"铝合金块","6061-T6","公斤",20]
[150,"《车铣复合加工技术》",80,"铝合金棒","6061-T6","公斤",20]
[151,"《车铣复合加工技术》",80,"钨钢铣刀/平底刀","5080-C ，4*11*50L*4TAH","只",4]
[152,"《车铣复合加工技术》",80,"钨钢铣刀/平底刀","5080-C ，6*16*50L*4TAH","只",4]
[153,"《车铣复合加工技术》",80,"钨钢铣刀/平底刀","5080-C ，8*20*60L*4TAH","只",4]
[154,"《数控多轴加工技术》",80,"专业级可调式扭力扳手","3/8#系列专业级可调式扭力扳手，扭力范围5-25Nm，加套筒10件套","只",1]
[155,"《数控多轴加工技术》",80,"专业级可调式扭力扳手","3/8#系列专业级可调式扭力扳手，扭力范围10-50Nm，加套筒10件套","只",1]
[156,"《数控多轴加工技术》",80,"虎钳测压力仪JM-PM1000","虎钳测压力仪JM-PM1000","只",1]
[157,"城市轨道交通运营管理",322,"尖嘴钳","160mm","把",1]
[158,"城市轨道交通运营管理",322,"剥线钳","0.2-6mm²","把",1]
[159,"城市轨道交通运营管理",322,"管型接线端子压线钳","0.25-10mm²","把",10]
[160,"城市轨道交通运营管理",322,"U 型压线钳","0.25-2.5mm²","把",1]
[161,"城市轨道交通运营管理",322,"斜口钳","0.25-2.5mm²","把",1]
[162,"城市轨道交通运营管理",322,"电动螺丝刀","9980FV塑箱2电","把",1]
[163,"城市轨道交通运营管理",322,"SV叉型绝缘端子","接0.5平的多芯铜线","颗",10000]
[164,"城市轨道交通运营管理",322,"VE管型绝缘端子","接0.5平的多芯铜线","颗",10000]
[165,"城市轨道交通运营管理",322,"剪刀","长17CM","把",4,"蓝色红色各2把"]
[166,"城市轨道交通运营管理",322,"鸭嘴剥线钳","通用","个",5]
[167,"城市轨道交通运营管理",322,"电工胶带","黑/红色","卷",10]
[168,"城市轨道交通运营管理",322,"多芯铜线（绿色）","0.50平","米",2000]
[169,"城市轨道交通运营管理",322,"多芯铜线（红色）","0.50平","米",2000]
[170,"城市轨道交通运营管理",322,"多芯铜线（黄色）","0.50平","米",1800]
[171,"城市轨道交通运营管理",322,"多芯铜线（黑色）","0.50平","米",1600]
[172,"城市轨道交通运营管理",322,"多芯铜线（蓝色）","0.50平","米",1800]
[173,"城市轨道交通运营管理",322,"号码管打印色带","TP70","只",15]
[174,"城市轨道交通运营管理",322,"号码管（黄色）","0.50平","卷",10,"100米/卷"]
[175,"城市轨道交通运营管理",322,"布基胶带","宽5cm*10米","卷",2,"白色"]
[176,"城市轨道交通运营管理",322,"多孔板","60cm*70cm","块",2,"带支架脚"]
[177,"城市轨道交通运营管理",322,"底座铁路信号继电器（带底座）",null,"只",20]
[178,"城市轨道交通运营管理",322,"电线接线端子分线盒","二进四出,尺寸：长66*宽38*高36","个",30,"二进四出"]
[179,"城市轨道交通运营管理",322,"焊锡丝","1.00mm*100克","卷",30]
[180,"城市轨道交通运营管理",322,"十字螺丝刀","4寸","把",20]
[181,"城市轨道交通运营管理",322,"烙铁（带烙铁架）","60W双温","把",10]
[182,"城市轨道交通运营管理",322,"空开","1P-10A","只",20]
[183,"城市轨道交通运营管理",322,"E10螺口小灯泡","3.8V","只",200]
[184,"城市轨道交通运营管理",322,"小车升弓电池","BT-HSE-38-12(12V38Ah/10HR)","包",4]
[185,"城市轨道交通运营管理",322,"稳压电源","MT-152D；输入：AC220V/50Hz；输出：DC0-15V,0-2A","只",6]
[186,"城市轨道交通运营管理",322,"内六角扳手","球头9件套","套",10]
[187,"城市轨道交通运营管理",322,"PPT翻页笔","充电型","支",2]
[188,"城市轨道交通运营管理",322,"电磁继电器（带底座）","12v；8脚","套",20]
[189,"城市轨道交通运营管理",322,"梅花（十字）螺丝刀","6mm*200mm","支",10]
[190,"城市轨道交通运营管理",322,"梅花（十字）螺丝刀","4mm*200mm","支",10]
[191,"城市轨道交通运营管理",322,"齿轮、链条、皮带三种传动教学实验仪器","金属制品","套",5]
[192,"城市轨道交通运营管理",322,"电动三开道岔模型W3-55225","W3-55225（1000mm*60mm）","个",2]
[193,"城市轨道交通运营管理",322,"票务管理用练功炒","面值100元；100张/扎","扎",50]
[194,"工业机器人应用系统集成",168,"自动交换夹具","OX系列NSK-03D/03DJ 工具侧","个",2]
[195,"工业机器人应用系统集成",168,"插排","米家智能插线板2 5位插孔版插座","个",2]
[196,"工业机器人应用系统集成",168,"制图工具板","绘图板实木板制图板A2号","个",2]
[197,"工业机器人应用系统集成",168,"HDMI分配器","HDMI分配器 一进二 SWR9101E/93 DC 5V","个",1]
[198,"工业机器人应用系统集成",168,"机器人联网路由","路由器 Q6（1母1子套装）","个",1]
[199,"工业机器人应用系统集成",168,"强弱电箱","电子电工五金工具套装 X1-F","个",1]
[200,"工业机器人应用系统集成",168,"安装工具箱","拆装工具套装 X3-ABG","个",1]
[201,"工业机器人应用系统集成",168,"电线卡扣","（SAMZHE）固线钉线卡墙钉 8mm 网线钉子电话线圆形钢钉网线布线家装扣钉 100只装 ZD-24","袋",4]
[202,"工业机器人应用系统集成",168,"电线卡扣","线器电线固定器免钉无痕线卡整理收纳走线夹网线卡子扣自粘神器","袋",4]
[203,"工业机器人应用系统集成",168,"pvc线槽","明装走线槽地面防踩自粘加厚网线电线槽阻燃绝缘5号/米","米",10]
[204,"自动化生产线安装调试",168,"信号放大器 ","可自动连接并放大Q6路由器wifi，长46.2mm；宽66.5mm；高102.5mm；支持Mesh；支持IPv6，内置天线；频段：双频","个",2]
[205,"自动化生产线安装调试",168,"气管接头","PL-L型螺纹二通，PL4M5","个",50]
[206,"自动化生产线安装调试",168,"气管","4*2.5mm","米",20]
[207,"自动化生产线安装调试",168,"吹尘枪","吹尘枪+9米弹簧管(带接头)","个",1]
[208,"自动化生产线安装调试",168,"螺丝刀","手电钻充电电动螺丝刀锂电钻工具箱套装电转打孔GSR120-LI，12v，有正/逆转向","个",1]
[209,"自动化生产线安装调试",168,"滑动气缸","TN10×75+DMSJ-2，配两个传感器","个",1]
[210,"自动化生产线安装调试",168,"空开带漏电保护器","西门子(SIEMENS) 空气开关 漏电保护断路器2P 63A 带漏保5SU93261CR63","个",2]
[211,"单片机技术应用",190,"此贴手持按钮控制盒","四位（急停+2自复+2档旋钮）","盒",2]
[212,"单片机技术应用",190,"机器人机械手臂三合一控制器","开源6路多级控制器 兼容ARDUINO/51/STM32 机器人机械手臂主板","套",1]
[213,"单片机技术应用",190,"5号电池","(NANFU)5号电池40粒 盒装","盒",4]
[214,"单片机技术应用",190,"单片机开发板",null,"个",1]
[215,"单片机技术应用",190,"7号电池","(NANFU)7号电池40粒 盒装","盒",4]
[216,"工业机器人离线编程与仿真",168,"插座","小米插线板(5孔位) 全长2米","个",4]
[217,"工业机器人离线编程与仿真",168,"HDMI分配器"," HDMI分配器 一进二 SWR9101E/93 DC 5V","个",2]
[218,"工业机器人离线编程与仿真",168,"电线","多股铜芯软电线AVR 0.75平，100m","卷",9]
[219,"工业机器人离线编程与仿真",168,"电线","多股铜芯软电线AVR 0.5平，100m","卷",9]
[220,"工业机器人离线编程与仿真",168,"电线","（CHNT） 电线电缆 BV2.5平方国 阻燃性能 2.5平方 ","卷",4]
[221,"工业机器人综合实训",168,"小型螺丝刀套装","吉米S2超硬加长45mm精密螺丝刀套装 ","个",1]
[222,"工业机器人综合实训",168,"网线","高速千兆网络连接线CAT6，50","卷",4]
[223,"工业机器人综合实训",168,"防静电手套","48-129Ansell耐磨防护PU涂掌劳保手套薄款工作尼龙夏季防静电，M号","双",10]
[224,"工业机器人综合实训",168,"TPU 材质耗材","1kg丝线材柔韧柔软耗材 透明橙色","卷",2]
[225,"工业机器人综合实训",168,"工业级交换机","TP-LINK TL-SF005工业级交换机（TL-SG2005【全电口】5口千兆网管型交换机","个",2]
[226,"工业机器人综合实训",168,"控制板","主控芯片采用IAP15W4K58S4，采用12V锂电池供电，3位数码管可实时显示电池电压，电机驱动芯片采用2块TB6612芯片驱动智能车4个车轮","个",1]
[227,"工业机器人综合实训",168,"工业机器人手指气缸","工业机器人SMC气动手指气缸MHZ2-16D","个",4]
[228,"工业机器人综合实训",168,"工业机器人手指气缸","工业机器人SMC气动手指气缸250D","个",4]
[229,"逆向工程",162,"显像剂","DPT-5","瓶",10]
[230,"逆向工程",162,"SD卡","DT100 G3 32G","个",4]
[231,"逆向工程",162,"标记点","内6mm外10mm低粘","1000点/个",2,"适配三维天下"]
[232,"3D打印技术",259,"PLA线材","白色/1KG/1.75","KG",10,"与现有设备相匹配"]
[233,"3D打印技术",259,"SLA用光敏树脂",null,"L",3,"白色标准V3"]
[234,"3D打印技术",259,"SLA用耗材盒",null,"个",2,"与现有设备相匹配"]
[235,"3D打印技术",259,"3D打印机润滑脂","10g/支","支",10,"软瓶装10g润滑脂"]
[236,"3D打印技术",259,"3D打印尖嘴钳",null,"把",5]
[237,"3D打印技术",259,"一次性擦拭布","20cm*20cm*100片","包",4]
["合计：82164.00元"]